[Strings.0409]
Msft                    = "Microsoft"
Realtek                 = "Realtek Semiconductor Corp."

VLanTagging             = "802.1Q/1p VLAN 标记"
;VLanID                 = "802.1Q VLAN ID"
ChecksumOffload         = "卸载校验和"
LargesendOffload        = "卸载 TCP_LargeSend"
SpeedDuplexMode         = "链接速度/双工模式"
auto_nego               = "自动协商"
sd10half                = "10Mbps/半双工"
sd10full                = "10Mbps/全双工"
sd100half               = "100Mbps/半双工"
sd100full               = "100Mbps/全双工"
sd1000full              = "1000Mbps/全双工"
NetworkAddress          = "网络地址"
JumboFrame              = "Jumbo 帧"
;TxDescNumber           = "Number of Tx Descriptor"
;RxDescNumber           = "Number of Rx Descriptor"
;TxHPQDescNumber        = "Number of High Priority Tx Descriptor"
WOLCapability           = "基于 ARP/PING 唤醒"
WOLLinkChange           = "唤醒链接更改"
LDPSCapability          = "链接关闭节能"
OptimalPerf             = "最佳性能"
FlowControl             = "流控制"
enable                  = "启用"
disable                 = "停用"
WakeUpOnLinkChange      = "唤醒链接更改"
LinkDownPowerSaving     = "链接关闭节能"
ReceiveBufferSize       = "接收缓冲区大小"
8Kbytes                 = "8K 字节"
16Kbytes                = "16K 字节"
32Kbytes                = "32K 字节"
64Kbytes                = "64K 字节"
WakeUpUsingAPMMode      = "使用 APM 模式唤醒"
NumberTxCoalesceBuffer  = "Tx 合并缓冲区数"
TaskOffload             = "任务卸载"
AllDisable              = "全部禁用"
checksum                = "检查和"
ChksumTCPSegment        = "Chksum 和 TCP_Segment"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
TxRxChecksum            = "Tx/Rx 校验和"
RxChecksum              = "Rx 校验和"
TxChecksum              = "Tx 校验和"
WakeUpOnARPPING         = "唤醒 ARP/PING"
TransmitDMABurstSize    = "传输 DMA 脉冲大小"
16bytes                 = "16 字节"
32bytes                 = "32 字节"
64bytes                 = "64 字节"
128bytes                = "128 字节"
256bytes                = "256 字节"
512bytes                = "512 字节"
1024bytes               = "1024 字节"
2048bytes               = "2048 字节"
ReceiveDMABurstSize     = "接收 DMA 脉冲大小"
Unlimitted              = "无限"
ReceiveFIFOthreshold    = "接收 FIFO 阈值"
NoThreshold             = "无阈值"

;;Source disk name
DiskDescription = "Realtek 10/100 NIC 系列 NDIS 驱动程序"

RTL8139.DeviceDesc        = "Realtek RTL8139/810x Family Fast Ethernet NIC"
RTL8139P.DeviceDesc       = "Realtek RTL8139C+ Fast Ethernet NIC"

RTL8139NetgearFA311.DeviceDesc   = "NETGEAR FA311v2 PCI Adapter"
RTL8139DLinkDFE690TXD.DeviceDesc = "D-Link DFE-690TXD CardBus Card"
RTL8139DLinkDFE538TX.DeviceDesc  = "D-Link DFE-538TX 10/100 Adapter"
RTL8139DLinkDFE530TX.DeviceDesc  = "D-Link DFE-530TX+ PCI Adapter"
RTL8139DLinkDFE528TX.DeviceDesc  = "D-Link DFE-528TX PCI Adapter"

RTL8139Panasonic.DeviceDesc = "(MOBILE ASSIST)Realtek RTL8139/810x Family Fast Ethernet NIC"

;;NT service name
Rtlnicxp.Service.DispName    = "Realtek 10/100 NIC 系列 NDIS x86 驱动程序"


