[strings.0409]
  MS=				  "Microsoft"
  PROVIDER=                       "Eicon Networks"
  PRIVITEMID_CARD=                "{2CD6D901-506B-11d1-BF23-00A0242DD63F}"
  DRVDIR=                         "disdn"

  DISERV_B8_V2_PCI_DISP=          "Eicon Diva Server 4BRI-8M 2.0 (PCI)"
  DISERV_V_B8_V2_PCI_DISP=        "Eicon Diva Server V-4BRI-8"
  DISERV_P30_V2_PCI_DISP=         "Eicon Diva Server PRI 2.0 (PCI)"
  DISERV_B2_PCI_V2_DISP=          "Eicon Diva Server BRI-2M 2.0 (PCI)"
  DISERV_V_B2_PCI_V2_DISP=        "Eicon Diva Server V-BRI-2"
  DISERV_B2F_PCI_V2_DISP=         "Eicon Diva Server 2FX"
  DISERV_P8_E1T1_V3_PCI_DISP=     "Eicon Diva Server PRI/E1/T1-8"
  DISERV_P24_T1_V3_PCI_DISP=      "Eicon Diva Server PRI/T1-24"
  DISERV_P30_E1_V3_PCI_DISP=      "Eicon Diva Server PRI/E1-30"
  DISERV_V_P_E1T1_V3_PCI_DISP=    "Eicon Diva Server PRI/E1/T1"
  DISERV_V_P24_T1_V3_PCI_DISP=    "Eicon Diva Server V-PRI/T1-24"
  DISERV_V_P30_E1_V3_PCI_DISP=    "Eicon Diva Server V-PRI/E1-30"
  DISERV_ANALOG_4PORT_DISP=       "Eicon Diva Server Analog-4P"
  DISERV_ANALOG_8PORT_DISP=       "Eicon Diva Server Analog-8P"
  DISERV_V_ANALOG_4PORT_DISP=     "Eicon Diva Server V-Analog-4P"
  DISERV_V_ANALOG_8PORT_DISP=     "Eicon Diva Server V-Analog-8P"
  DISERV_COMBINED_DISP=           "Eicon Diva Server Combined Adapter"

  ; friendly server names
  DIVA_DISP=                      "Eicon Driver for all DIVA PnP cards"
  DIVASRV_DISP=                   "Eicon Driver for all Diva Server PnP cards"
  DIVACO_DISP=                    "Eicon Connection Oriented Driver for all Diva PnP cards"
  DIVACOSRV_DISP=                 "Eicon Connection Oriented Driver for all Diva Server PnP cards"
  MAINT_DISP=                     "Eicon Maintenance Driver"
  CAPI_DISP=                      "Eicon CAPI 2.0 Driver"
  CAPI20=                         "CAPI20"

  SERVER_DISK_1_LABEL=			  "Diva Server for Windows Setup"

  ; registry data types
  ;     types with NCLOB don't overwrite existing values
  REG_SZ=                         0x00000000
  REG_SZ_NCLOB=                   0x00000002
  REG_MSZ=                        0x00010000
  REG_MSZ_NCLOB=                  0x00010002
;  REG_MSZ_APPEND=                 0x0001000A
;  REG_MSZ_DELVAL=                 0x00010006
  REG_ESZ=                        0x00020000
  REG_DW=                         0x00010001
  REG_DW_NCLOB=                   0x00010003

  ; bus types [ USB isn't existing, fake as Internal (or PCI)? ]
  PCI=                            5

  ; device characteristics
;  NCF_VIRTUAL=                    0x0001
  NCF_PHYSICAL=                   0x0004
;  NCF_HIDDEN=                     0x0008

;***************************************************
; Supported Switch Types for Server cards:
;  [ISDN_SWITCH_AUTO(0x01)] | ISDN_SWITCH_ATT(0x02
;  ISDN_SWITCH_NI1(0x04)    | ISDN_SWITCH_NTI(0x08)
;  ISDN_SWITCH_INS64(0x10)  | ISDN_SWITCH_1TR6(0x20)
;  ISDN_SWITCH_VN3(0x40)    | ISDN_SWITCH_DSS1(0x80)
;  ISDN_SWITCH_AUS(0x100)   | ISDN_SWITCH_BEL(0x200)
;  ISDN_SWITCH_SWE(0x1000)  | ISDN_SWITCH_ITA(0x2000)
;  ISDN_SWITCH_TWN(0x4000)
;***************************************************
  GENERIC_ISDNSWITCHTYPES=  0x73DE

; card trace masks
  BASIC_CARD_MASK=          0x00000031
  BASIC_CARD_POTS_MASK=     0x00030031

;*** end *********************************************************************

